Tentative field-widened, temperature compensated, 1064 nm, Michelson Specifications:

Wavelength = 1064 nm

FSR = 1 GHz

Clear aperture = 20 mm

Maximum field of view = 2 mrad

1 FSR tuning for delta-T < 10 and >5 degree C

Off-axis design providing access to beam reflected back towards source